Cold-rolled product

|  |  |  |
| --- | --- | --- |
| **Steel type** | **Steel grade** | **Application** |
|
| Cold harden coil | SPCC-1B、SPCC-1D、SPCD-1B、SPCD-1D、SPCE-1B、SPCE-1D | - |
| Cold-rolled low carbon steel | DC01 | Common |
| DC03 | Drawing |
| DC04 | Deep drawing |
| DC05 | Special deep drawing |
| DC06 | Ultra deep drawing |
| Phosphorus high strength steel | P175 | Drawing |
| P205 | Common |
| P250 | Structure |
| Baked harden steel | CR140BH | Deep drawing |
| CR180BH | Deep drawing or drawing |
| CR220BH | Drawing or common |
| CR260BH | Common or structure |
| CR300BH | Structure |
| Flux-cored wire steel | HS1、HS2、HS3 | Flux-core |
| Carbon structural steel | 08Al | Drawing or common |
| 10、20、30、40、50 | Structure |
| Low-alloy structural steel | HC260LA | Structure |
| HC300LA |
| HC340LA |
| HC380LA | Structure or intensity structure |
| HC420LA |
| Battery shell steel | DCK | Automobile battery shell |
| Hot-rolled section steel | 1500HS | Automobile structural component |
| Sliding rail steel | S245G | For sliding rail |